|  |  |  |
| --- | --- | --- |
|  | SCHEDULE B - QUOTATION |  |

RFQ Title: Supply and Delivery of Five (5) [More or Less] Tandem Axle Dump Trucks Complete with Dump Box, Trailer Hitch, Snow Plough, and Salt Spreader

RFQ No: 1220-040-2019-079

**CONTRACTOR**

**Legal Name:**

**Contact Person and Title:**

**Business Address:**

**Business Telephone:**

**Business Fax:**

**Business E-Mail Address:**

**CITY OF SURREY**

TO:

City Representative: Richard D. Oppelt, Manager Procurement Services

Address: Surrey City Hall

Finance & Technology Department – Purchasing Section

Reception Counter, 5th Floor West

13450 – 104th Avenue, Surrey, B.C., V3T 1V8

Telephone: 604-590-7274

Email: purchasing@surrey.ca

1. The Contractor offers to supply to the City of Surrey the Goods for the prices plus applicable taxes as follows:

Year, Make & Model: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

All costs to meet the preferred specifications shall be included in the following delivered prices.

|  |  |  |
| --- | --- | --- |
| **F.O.B.**DestinationFreight Prepaid | **Payment Terms:**A cash discount of \_\_\_\_% will be allowed if invoices are paid within \_\_\_ days, or the \_\_\_ day of the month following, or net 30 days, on a best effort basis. | **Ship Via:** |
| **Item** | **Particulars** |  | **Cost per Unit (CDN $)** |
| 1 | Price per Unit: | Note: Provide price and quantity where price breaks are applicableQuantity:Price per Unit: | $ |
| 2 | Province of B.C. Environmental Levy (Battery): | $ |
| 3 | Province of B.C. Advance Disposal Fee (Tires): | $ |
| 4 | Air Conditioning Surcharge: | $ |
| 5 | Accessories quote |  |
|  |  a.) Langfab | $ |
|  |  b.) Vimar | $ |
|  |  c.) Commercial Truck | $ |
| 6 | Subtotal: | $ |
| 7 | GST (5%) on $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | $ |
| 8 | PST (7%) on $\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | $ |
| 9 | **TOTAL QUOTATION PRICE FOR ONE UNIT:** | $ |
| *Pricing is firm until (state date):*  |
| *ALL PRICING IN CANADIAN DOLLARS* |

**The completed unit shall be delivered within \_\_\_\_\_\_\_ days after receipt of purchase order.**

Manufacturer’s Warranty: State Warranty

Body Warranty: State Warranty\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Warranty repairs shall be performed at

Please complete if applicable: British Columbia Certified

2. In addition to the warranties provided in the Draft Quotation Agreement, this Quotation includes the following warranties:

3. I/We have reviewed the RFQ Attachment 1, Schedule A – Specifications of Goods and if requested by the City, I/we would be prepared to meet those requirements, amended by the following departures and additions (list, if any):

**Requested Departure(s) / Alternative(s) / Addition(s)**

The City is not obligated to accept any alternatives. The City will determine what constitutes acceptable deviations and overall best value.

4. If this Quotation is accepted by the City, a contract will be created as described in:

(a) the Agreement;

(b) the RFQ; and

(c) other terms, if any, that are agreed to by the parties in writing.

5. Capitalized terms used and not defined in this Quotation will have the meanings given to them in the RFQ. Except as specifically modified by this Quotation, all terms, conditions, representations, warranties and covenants as set out in the RFQ will remain in full force and effect.

6. I/We have reviewed the RFQ Attachment 1 – Draft Quotation Agreement. If requested by the City, I/we would be prepared to enter into that Agreement, amended by the following departures (list, if any):

**Section Requested Departure(s) / Alternative(s)**

7. I/We the undersigned duly authorized representatives of the Contractor, having received and carefully reviewed the RFQ including without limitation the specifications and the General Terms and Conditions, submit this Quotation in response to the RFQ.

**This Quotation** is offered by the Contractor this \_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, 201\_.

**CONTRACTOR**

**I/We have the authority to bind the Contractor**

|  |  |
| --- | --- |
| \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(Legal Name of Contractor)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(Signature of Authorized Signatory)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(Print Name and Position of Authorized Signatory) | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(Signature of Authorized Signatory)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(Print Name and Position of Authorized Signatory) |

## SCHEDULE B-1 – PREFERRED TECHNICAL SPECIFICATIONS RESPONSE FORM

**PROJECT TITLE: Supply and Delivery of Five (5) [More or Less] Tandem Axle Dump Trucks Complete with Dump Box, Trailer Hitch, Snow Plough, and Salt Spreader**

**PROJECT No.: 1220-040-2019-079**

The specification herein states the preferred requirements of the City of Surrey. All Quotations shall be regular in every respect. Unauthorized conditions, limitations, or provisions may be cause for rejection. The City of Surrey will consider as "irregular" or "non-responsive" any Quotation not prepared and submitted in accordance with the RFQ document and specification, or any Quotation lacking sufficient technical literature to enable the City to make a reasonable determination of compliance to the specification.

It shall be the Contractor's responsibility to carefully examine each item of the specification. Failure to offer a completed Quotation or failure to respond to each section of the technical specification may cause the Quotation to be rejected without review as "non-responsive". All variances, exceptions and/or deviations shall be fully described in the appropriate section.

Note: Contractors are directed to list complete manufacturers’ details of model proposed in the right-side column under manufacturers’ specifications.

| **Preferred** **Specifications** | **Yes****(Circle)** | **No****(Circle)** | **Manufacturers’ Specifications of Equipment Offered. Contractor to indicate compliance or deviation with specifications below.** |
| --- | --- | --- | --- |
| 1. **EXTERIOR**
 |
| 1. Weight GVWR. 27,000 kgs approx., GCWR shall be no less than 50,000 kgs
 | Y | N |  |
| 1. Wheelbase 220” approx. (To fit a 16’6” Dump Box approx.) Allow for hydraulic tank between cab and dump box. Please provide details. Chassis provider to confirm with Langfab/Commercial Truck Equipment for optimal wheelbase
 | Y | N |  |
| 1. Bumper: Front Only, Painted black, full width, c/w two tow hooks
 | Y | N |  |
| 1. Mirrors (Power): Two outside west coast style, heat control switched from inside cab, stainless steel backs, c/w 2 auxiliary convex mirrors attached to main mirrors, one each side
 | Y | N |  |
| 1. All lights to comply with Provincial Laws.

 **Front:** hi/lo beam headlightsLights (LED lights only) 4 - way hazards and directional lamps, cab ID lights ID lights on mirrors.Additional switching and wiring for snow plough lighting package **(lights included in pricing from Commercial Truck Equipment)** **Rear lights: (included in dump box package)**combination stop/turn  Separate hazard lights License plate light All lights shock mountedTwo additional reverse lights mounted either side of tow hitch  | Y | N |  |
| 1. Colour:

 Bright White | Y | N |  |
| 1. Cab:

 Conventional style Tilt hood Stationery grill | Y | N |  |
| 1. Mud Flaps, behind front wheels, behind and in front of tandem axles
 | Y | N |  |
| 1. Running Boards, Step tanks r/side with boot brush, Steps on left side including boot brush
 | Y | N |  |
| 1. Cab mounted grab handles in suitable positions for ease of access and egress – both sides
 | Y | N |  |
| 1. Audible B/U Alarm, Grote part # 73040 97 dBA
 | Y | N |  |
| 1. Vertical Exhaust, with muffler guard, and guarding around any exposed pipe which could pose a burn hazard
 | Y | N |  |
| 1. Cab drip moldings
 | Y | N |  |
| 1. Fuel Tank – Polished aluminum, capacity – 100 gal
 | Y | N |  |
| 1. Horns, Dual outside roof mounted air horns, with dual electric
 | Y | N |  |
| 1. Right side lower door visibility window
 | Y | N |  |
| 1. ABS and trailer light wiring to rear of chassis
 | Y | N |  |
| 1. Two beacon lights mounted on dump box – LED amber Whelen (R2LPPA),
 | Y | N |  |
| 1. Corrosion protection of frame (after market treatment). Cab protection shall be also be applied – please provide details of offering
 | Y | N |  |
| 1. **INTERIOR & INSTRUMENTS**
 |
| 1. Seats (2) – With Arm Rests, Air ride type with high back, cloth seat with seat covers, Air controlled, Air ride
 | Y | N |  |
| 1. Heater/Defroster/Air Conditioning, Multiple speed fan
 | Y | N |  |
| 1. Wipers / Washers, intermittent type / 12 volt electric,
 | Y | N |  |
| 1. Visor, Outside mounted on cab, two padded inside cab
 | Y | N |  |
| 1. Lights, Interior dome operated by doors and switch
 | Y | N |  |
| 1. Instruments:

Full instrumentation as standard on bid model, engine low level alarm system, tach. Required, engine hour meter, outside temp. sensor, gauges as opposed to lights | Y | N |  |
| 1. Controls, Hand throttle – electronic
 | Y | N |  |
| 1. Power windows both sides
 | Y | N |  |
| 1. Floor Mats, One driver, one passenger, full insulated rubber mats
 | Y | N |  |
| 1. An aluminum storage box shall be fitted between the drivers and passengers’ seats for the driver store items. The box shall not interfere with any of the driver controls include gear shift, IQAN and Epoke control displays. A cup holder shall also be attached to the storage box
 | Y | N |  |
| 1. Radio/CB, AM/FM Stereo with Bluetooth capability, 40 Channel CB
 | Y | N |  |
| 1. Road temperature sender unit mounted on driver’s side mirror or similar with dash mounted gauge
 | Y | N |  |
| **C. CHASSIS, SUSPENSION, AXLES AND BRAKES** |
| 1. Axle Capacities:

 **Front:** Axle @ 20,000 lbs. Set back **Rear:** Meritor RT-46-164 @ 46,000 lbs. Rear ratio approx. 4.50 Hendrickson rear suspension Driver controlled diff lock and inter-axle lock Synthetic oil filled | Y | N |  |
| 1. Brakes (all air operated) – Anti-Lock

 **Front:** Meritor cam 16.5 x 6 QT-plus Drums Auto slacks C/R seals **Rear:** Meritor cam 16.5 x 7 QT-plus Drums Auto slacks C/R seals Maxi 30/30 pots Air system c/w air dryer/heater, 15 cu. ft. Compressor, all tanks, gauges, etc. to meet provincial standards. | Y | N |  |
| 1. Springs:

 **Front:** 20,000 lb. – Tapered Leaf provide details **Rear:** 46,000 lb. Hendrickson RTE 460 rear suspension provide details | Y | N |  |
| 1. Frame (front frame extension for snow plough)

 High tensile steel single frame rail Bolted Straight rail, Steel cross membersProvide details | Y | N |  |
| 1. The frame rail shall be clear from behind the cab, with inboard air tanks
 | Y | N |  |
| 1. **WHEELS, TIRES & STEERING**
 |
| 1. Tires (Michelin Only)

 Front: 2 @ 445R 22.5 18 Ply Steer type tread XZY Rear: 8 @ 11R 22.5 14 Ply X Multi D | Y | N |  |
| 1. Wheels (Budd Style):

 **Front:** 22.5 x 12.25 Alcoa Disc (2) **Rear:** 22.5 x 8.25 Alcoa Disc (8) | Y | N |  |
| 1. Steering (Tilt/Telescopic)

 Power Steering / Power Assisted Dual Steering Boxes | Y | N |  |
| 1. **ENGINE & TRANSMISSION**
 |
| 1. Engine:

To meet or exceed the latest engine emission standards.450 HP (approx.) Electronic controlled1650 ft./lb. torquePeak torque 1650 @ 900 rpm Jake Brake, cab controlled, 3 stageRacor 900 FG3122 fuel/water separatorProvide engine spec details - options | Y | N |  |
| 1. Engine to run rear mounted engine driven PTO piston pump capable 30 gpm @ 1800 rpm (pump supplied by Commercial Truck Equipment)
 | Y | N |  |
| 1. Cooling System:

HD radiatorFan clutch manual on/offLong life coolantAll silicone hosesBlock heater (110V electric) | Y | N |  |
| 1. Alternator:

 Minimum 160 amp 12 Volt | Y | N |  |
| 1. Starter:

 12 VoltDelco Remy | Y | N |  |
| 1. Battery:

 Minimum 3 – 12 Volt 3300 CCA total Night switch Covered battery compartment – polished aluminum | Y | N |  |
| 1. Allison 4500 RDS series

Synthetic oil filledProvide specs | Y | N |  |
| 1. Transmission:

 c/w transmission temp. gauge c/w cooler | Y | N |  |
| 1. Meritor MXL 18T driveline
 | Y | N |  |
| 1. **FILTERS, BELTS AND SERIAL NUMBERS**
 |
| 1. Filters: All filters for the first major service for complete truck.
 | Y | N |  |
| 1. Belts:

 List all belts used on truck. | Y | N |  |
| 1. Serial Numbers:

 List all serial numbers other than truck ID number and what each serial number pertains to. | Y | N |  |
| 1. **TRAINING**
 |
| 1. At dealer expense, provide training for drivers (1 per truck) and training for mechanic (2 days). All expenses paid by dealer.
 | Y | N |  |
| 1. Provide the City of Surrey with access to diagnostic software to trouble shoot and repair faults
 | Y | N |  |
| 1. **STANDARDS**
 |
| 1. Good must comply with government regulations and requirements:
* Federal Government Motor Vehicle Standards
* BC Motor Vehicle Act and Regulations
* BC Workers’ Compensation Board Regulations
* BC Emissions Standards
* Good shall be delivered with CVIP
* Good shall be delivered, plated and insured through the City of Surrey’s Insurance Broker
 | Y | N |  |
| 1. **STANDARD WARRANTY (provide details)**
 |
| 1. Engine
2. Power Train
3. Chassis
4. Corrosion
 | Y | N |  |
| 1. **EXTENDED WARRANTY (provide specific details & costs),**

 **MISCELLANEOUS** |
| 1. Extended warranty for:
* Engine,
* Engine emission components
* Transmission, power train
* Chassis
* Dump Box
 | Y | N |  |
| 1. Operators Manuals / Service Manuals

 1 – Service manual or CD c/w softwareA build sheet shall be provided detailing (but not limited to the following):* VIN
* Engine details including serial number
* Transmission details including serial number
* Diff details including serial number
* Oil types and quantities for all components
* Tire make, type and size
* Engine belts details
* Filter list for all components
* Battery details
* Beacon light make
* Body and hydraulic components
* Salt Spreader
* Snow Plough
 | Y | N |  |
| 1. Keys: 3 sets with each unit
 | Y | N |  |
| 1. Number One First Aid Kit (Hard Case)
 | Y | N |  |
| 1. 5 lb. Fire Extinguisher – Mounted
 | Y | N |  |
| 1. **Dump Box and Accessories**
 |
| 1. Aluminum box 16.6 foot long with high lift- tailgate as per **Langfab** quote
 | Y | N |  |
| 1. **IQAN Hydraulic System, front mount plough, underbody plough**
 |
| 1. As per **Commercial Truck Equipment Co**. quote
 | Y | N |  |
| 1. **Epoke Salt Spreader**
 |
| 1. Epoke Salt Spreader including installation as per **Vimar** quote
 | Y | N |  |
| 1. **Options**
 |
| 1. Contractors to provide a list of options and pricing as an addendum to the main pricing schedule
 | Y | N |  |