|  |  |  |
| --- | --- | --- |
|  | SCHEDULE B – FORM OF QUOTATION |  |

**RFQ Title: Supply and Delivery of Two (More or Less) Mini Skid Steer Stand-on**

 **Tracked Loaders**

**RFQ No.: 1220-040-2021-054**

**CONTRACTOR**

**Legal Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Contact Person and Title:**

**Business Address:**

**Business Telephone:**

**Business Fax:**

**Business E-Mail Address:**

TO:

**CITY OF SURREY**

City Representative: Richard D. Oppelt, Manager, Procurement Services

Email: purchasing@surrey.ca

If this offer is accepted by the City, such offer and acceptance will create a contract as described in:

(a) the RFQ;

(b) the specifications of Goods set out above and in Schedule A;

(c) the General Terms and Conditions; and

(d) this Quotation; and

(e) other terms, if any, that are agreed to by the parties in writing.

Capitalized terms used and not defined in this Quotation will have the meanings given to them in the RFQ. Except as specifically modified by this Quotation, all terms, conditions, representations, warranties and covenants as set out in the RFQ will remain in full force and effect.

I/We have reviewed the RFQ Attachment 1 – Quotation Agreement - Goods. If requested by the City, I/we would be prepared to enter into that Agreement, amended by the following departures (list, if any):

**Section Requested Departure(s) / Alternative(s)**

 **Please State Reason For Departure(s):**

**Changes and Additions to Specifications:**

In addition to the warranties provided in Attachment 1 – Quotation Agreement - Goods, this Quotation includes the following warranties:

I/We have reviewed the RFQ Attachment 1 – Quotation Agreement - Goods, Schedule A – Specifications of Goods. If requested by the City, I/we would be prepared to meet those requirements, amended by the following departures (list, if any):

**Section Requested Departure(s) / Alternative(s) / Additions**

 **Please State Reason For Departure(s):**

**Fees and Payments**

The Contractor offers to supply to the City of Surrey the Goods for the prices plus applicable taxes as follows:

Year, Make & Model:

All costs to meet the preferred specifications shall be included in the following delivered prices.

|  |  |  |
| --- | --- | --- |
| **F.O.B.**Destination | **Payment Terms**:A cash discount of \_\_\_\_% will be allowed if invoices are paid within \_\_\_ days, or the \_\_\_ day of the month following, or net 30 days, on a best effort basis. | **Ship Via:**Freight Prepaid |
| **Item** | **Item Name****(Description and Specifications)** | **(A)** | **(B)** | **(C)** |
| **Quantity** | **Unit Price** | **Total Amount****A x B = C** |
| 1. | Price  | 2 | $ | $ |
| 2 | Province of B.C. Environmental Levy (Battery): | $ | $ |
| 3 | Province of B.C. Advance Disposal Fee (Tires): | $ | $ |
| 4 | Air Conditioning Surcharge: | $ | $ |
| 5 | Other Fees/Levies (please state): |  | $ | $ |
| a.) |  | $ | $ |
| b.) |  | $ | $ |
| c.) |  | $ | $ |
| **CURRENCY: All Pricing in Canadian Dollars** | Subtotal: | $ |
| Price discount for Quantity 2: | - $ |
| GST (5%): | $ |
| PST (7%): | $ |
| **Total Price:** | **$** |
| ***Pricing is firm until (state date):*** |  |  |

**The completed unit shall be delivered within days after receipt of purchase order.**

Manufacturer’s Warranty: State Warranty

Warranty repairs shall be performed at

Please complete if applicable: British Columbia Certified

In addition to the warranties provided in the Draft Quotation Agreement, this Quotation includes the following warranties:

I/We the undersigned duly authorized representatives of the Contractor, having received and carefully reviewed the RFQ including without limitation the draft Agreement submit this Quotation in response to the RFQ.

**This Quotation** is offered by the Contractor this day of  , 2021.

**CONTRACTOR**

I/We have the authority to bind the Contractor:

(Full Legal Name of Contractor)

(Signature of Authorized Signatory)

(Print Name and Position of Authorized Signatory)

SCHEDULE B-1 – PREFERRED TECHNICAL SPECIFICATIONS RESPONSE FORM

The specification herein states the preferred requirements of the City of Surrey. All Quotations shall be regular in every respect. Unauthorized conditions, limitations, or provisions may be cause for rejection. The City of Surrey will consider as "irregular" or "non-responsive" any Quotation not prepared and submitted in accordance with the RFQ document and specification, or any Quotation lacking sufficient technical literature to enable the City to make a reasonable determination of compliance to the specification.

It shall be the Contractor's responsibility to carefully examine each item of the specification. Failure to offer a completed Quotation or failure to respond to each section of the technical specification may cause the Quotation to be rejected without review as "non-responsive". All variances, exceptions and/or deviations shall be fully described in the appropriate section.

**Note:** Contractors are directed to list complete manufacturers’ details of model proposed in the right-side column under manufacturers’ specifications.

|  |  |  |  |
| --- | --- | --- | --- |
| **Preferred Specifications** | **Yes****(Circle)** | **No****(Circle)** | **Manufacturers’ Specifications of Equipment Offered. Contractor to indicate compliance or deviation with specifications below.**  |
| 1. **General Specifications**
 |
| 1. Provide make and model details
 | Y | N |  |
| 1. Hinge pin height should be approximately 83 inches to allow the machine to load trucks
 | Y | N |  |
| 1. Machine should have a tipping capacity of approximately 2600 lbs
 | Y | N |  |
| 1. Machine rated operating capacity of approximately 900 lbs
 | Y | N |  |
| 1. Operating height with standard bucket should be approximately 105 inches
 | Y | N |  |
| 1. Overall length of machine should be 86 inches excluding any attachments
 | Y | N |  |
| 1. Machine should come with 7 inch rubber tracks, with a track length of approximately 43 inches
 | Y | N |  |
| 1. Overall width of machine should be approximately 36 inches to transverse narrow pathways and tracks
 | Y | N |  |
| 1. Machine to be supplied with standard bucket
 | Y | N |  |
| 1. Ground pressure – approximately 5 psi
 | Y | N |  |
| 1. **Engine**
 |
| 1. 3 - cylinder diesel engine, with a minimum of 24 hp.
 | Y | N |  |
| 1. Engine shall meet or exceed engine emission compliance for EPA Tier 4
 | Y | N |  |
| 1. Engine displacement of approximately 1.1 litre
 | Y | N |  |
| 1. Engine cooling system to -30F
 | Y | N |  |
| 1. 12 volt electrical system with battery capacity of approximately 800 amps cold crank
 | Y | N |  |
| 1. **Power Train**
 |
| 1. Hydraulics, flow rate 12 gpm, @ 3000 psi
 | Y | N |  |
| 1. Ground speed – approximately forward/reverse 4 mph
 | Y | N |  |
| 1. **Miscellaneous**
 |
| 1. Please provide a list of available attachments and price for the machine
 | Y | N |  |
| 1. Provide warranty details
 | Y | N |  |
| 1. Provide a full set of filters
 | Y | N |  |
| 1. Provide oil details, specifications, and quantity
 | Y | N |  |
| 1. Supply operator’s manual, service manual and spare parts manual
 | Y | N |  |
| 1. Location of local service facility in Surrey or close proximity
 | Y | N |  |
| 1. Contractor to provide operator orientation training and training to City mechanical staff
 | Y | N |  |
| 1. Provide details of optional attachments, including pricing
 |  |  |  |